Lab - Configure Network Devices with SSH (Instructor Version)

**Instructor Note**: Red font color or gray highlights indicate text that appears in the instructor copy only.

# Topology



# Addressing Table

| Device | Interface | IP Address | Subnet Mask | Default Gateway |
| --- | --- | --- | --- | --- |
| R1 | G0/0/1 | 192.168.1.1 | 255.255.255.0 | N/A |
| S1 | VLAN 1 | 192.168.1.11 | 255.255.255.0 | 192.168.1.1 |
| PC-A | NIC | 192.168.1.3 | 255.255.255.0 | 192.168.1.1 |

# Objectives

Part 1: Configure Basic Device Settings

Part 2: Configure the Router for SSH Access

Part 3: Configure the Switch for SSH Access

Part 4: SSH from the CLI on the Switch

# Background / Scenario

In the past, Telnet was the most common network protocol used to remotely configure network devices. Telnet does not encrypt the information between the client and server. This allows a network sniffer to intercept passwords and configuration information.

Secure Shell (SSH) is a network protocol that establishes a secure terminal emulation connection to a router or other networking device. SSH encrypts all information that passes over the network link and provides authentication of the remote computer. SSH is rapidly replacing Telnet as the remote login tool of choice for network professionals. SSH is most often used to log in to a remote device and execute commands. However, it can also transfer files using the associated Secure FTP (SFTP) or Secure Copy (SCP) protocols.

The network devices that are communicating must be configured to support SSH in order for SSH to function. In this lab, you will enable the SSH server on a router and then connect to that router using a PC with an SSH client installed. On a local network, the connection is normally made using Ethernet and IP.

**Note**: The routers used with CCNA hands-on labs are Cisco 4221 with Cisco IOS XE Release 16.9.4 (universalk9 image). The switches used in the labs are Cisco Catalyst 2960s with Cisco IOS Release 15.2(2) (lanbasek9 image). Other routers, switches, and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and the output produced might vary from what is shown in the labs. Refer to the Router Interface Summary Table at the end of the lab for the correct interface identifiers.

**Note**: Make sure that the routers and switches have been erased and have no startup configurations. If you are unsure, contact your instructor.

**Instructor Note**: Refer to the Instructor Lab Manual for the procedures to initialize and reload devices.

# Required Resources

* 1 Router (Cisco 4221 with Cisco IOS XE Release 16.9.4 universal image or comparable)
* 1 Switch (Cisco 2960 with Cisco IOS Release 15.2(2) lanbasek9 image or comparable)
* 1 PC (Windows with a terminal emulation program, such as Tera Term)
* Console cables to configure the Cisco IOS devices via the console ports
* Ethernet cables as shown in the topology

# Instructions

## Configure Basic Device Settings

In Part 1, you will set up the network topology and configure basic settings, such as the interface IP addresses, device access, and passwords on the router.

### Cable the network as shown in the topology.

### Initialize and reload the router and switch.

### Configure the router.

Open configuration window

* + - 1. Console into the router and enable privileged EXEC mode.

router> **enable**

* + - 1. Enter configuration mode.

router# **configure terminal**

* + - 1. Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.

router(config)# **no ip domain-lookup**

* + - 1. Assign **class** as the privileged EXEC encrypted password.

router(config)# **enable secret class**

* + - 1. Assign **cisco** as the console password and enable login.

router(config)# **line console 0**

router(config-line)# **password cisco**

router(config-line)# **login**

* + - 1. Assign **cisco** as the VTY password and enable login.

router(config)# **line vty 0 4**

router(config-line)# **password cisco**

router(config-line)# **login**

* + - 1. Encrypt the plaintext passwords.

router(config)# **service password-encryption**

* + - 1. Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.

router(config)# **banner motd $ Authorized Users Only! $**

* + - 1. Configure and activate the G0/0/1 interface on the router using the information contained in the Addressing Table.

router(config)# **interface g0/0/1**

router(config-if)# **ip address 192.168.1.1 255.255.255.0**

router(config-if)# **no shutdown**

* + - 1. Save the running configuration to the startup configuration file.

router# **copy running-config startup-config**

### Configure PC-A.

* + - 1. Configure PC-A with an IP address and subnet mask.
      2. Configure a default gateway for PC-A.

### Verify network connectivity.

Ping R1 from PC-A. If the ping fails, troubleshoot the connection.

Close configuration window

## Configure the Router for SSH Access

Using Telnet to connect to a network device is a security risk because all the information is transmitted in a clear text format. SSH encrypts the session data and provides device authentication, which is why SSH is recommended for remote connections. In Part 2, you will configure the router to accept SSH connections over the VTY lines.

### Configure device authentication.

The device name and domain are used as part of the crypto key when it is generated. Therefore, these names must be entered prior to issuing the **crypto key** command.

Open configuration window

* + - 1. Configure device name.

router(config)# **hostname R1**

* + - 1. Configure the domain for the device.

R1(config)# **ip domain-name ccna-lab.com**

### Configure the encryption key method.

R1(config)# **crypto key generate rsa modulus 1024**

The name for the keys will be: R1.ccna-lab.com

% The key modulus size is 1024 bits

% Generating 1024 bit RSA keys, keys will be non-exportable...

[OK] (elapsed time was 1 seconds)

R1(config)#

\*Jan 28 21:09:29.867: %SSH-5-ENABLED: SSH 1.99 has been enabled

### Configure a local database username.

Configure a username using **admin** as the username and **Adm1nP@55** as the password.

R1(config)# **username admin secret Adm1nP@55**

### Enable SSH on the VTY lines.

* + - 1. Enable Telnet and SSH on the inbound VTY lines using the **transport input** command.

R1(config)# **line vty 0 4**

R1(config-line)# **transport input telnet ssh**

* + - 1. Change the login method to use the local database for user verification.

R1(config-line)# **login local**

R1(config-line)# **end**

### Save the running configuration to the startup configuration file.

R1# **copy running-config startup-config**

Destination filename [startup-config]?

Building configuration...

[OK]

R1#

### Establish an SSH connection to the router.

* + - 1. Start Tera Term from PC-A.
      2. Establish an SSH session to R1. Use the username **admin** and password **Adm1nP@55**. You should be able to establish an SSH session with R1.

Close configuration window

## Configure the Switch for SSH Access

In Part 3, you will configure the switch to accept SSH connections. After the switch has been configured, establish an SSH session using Tera Term.

### Configure the basic settings on the switch.

Open configuration window

* + - 1. Console into the switch and enable privileged EXEC mode.

switch> **enable**

* + - 1. Enter configuration mode.

switch# **configure terminal**

* + - 1. Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.

switch(config)# **no ip domain-lookup**

* + - 1. Assign **class** as the privileged EXEC encrypted password.

switch(config)# **enable secret class**

* + - 1. Assign **cisco** as the console password and enable login.

switch(config)# **line console 0**

switch(config-line)# **password cisco**

switch(config-line)# **login**

* + - 1. Assign **cisco** as the VTY password and enable login.

switch(config)# **line vty 0 15**

switch(config-line)# **password cisco**

switch(config-line)# **login**

* + - 1. Encrypt the plain text passwords.

switch(config)# **service password-encryption**

* + - 1. Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.

switch(config)# **banner motd $ Authorized Users Only! $**

* + - 1. Configure and activate the VLAN 1 interface on the switch according to the Addressing Table.

switch(config)# interface vlan 1

switch(config-if)# **ip address 192.168.1.11 255.255.255.0**

switch(config-if)# **no shutdown**

* + - 1. Save the running configuration to the startup configuration file.

Switch# **copy running-config startup-config**

### Configure the switch for SSH connectivity.

Use the same commands that you used to configure SSH on the router in Part 2 to configure SSH for the switch.

* + - 1. Configure the device name as listed in the Addressing Table.
      2. Configure the domain for the device.

S1(config)# **ip domain-name ccna-lab.com**

* + - 1. Configure the encryption key method.

S1(config)# **crypto key generate rsa modulus 1024**

* + - 1. Configure a local database username.

S1(config)# **username admin secret Adm1nP@55**

* + - 1. Enable Telnet and SSH on the VTY lines.

S1(config)# **line vty 0 15**

S1(config-line)# **transport input telnet ssh**

* + - 1. Change the login method to use the local database for user verification.

S1(config-line)# **login local**

S1(config-line)# **end**

### Establish an SSH connection to the switch.

Start Tera Term from PC-A, and then SSH to the SVI interface on S1.

#### Question:

Are you able to establish an SSH session with the switch?

Type your answers here.

Yes. SSH can be configured on a switch using the same commands that were used on the router.

Close configuration window

## SSH From the CLI on the Switch

The SSH client is built into the Cisco IOS and can be run from the CLI. In Part 4, you will SSH to the router from the CLI on the switch.

### View the parameters available for the Cisco IOS SSH client.

Open configuration window

Use the question mark (**?**) to display the parameter options available with the **ssh** command.

S1# **ssh ?**

-c Select encryption algorithm

-l Log in using this user name

-m Select HMAC algorithm

-o Specify options

-p Connect to this port

-v Specify SSH Protocol Version

-vrf Specify vrf name

WORD IP address or hostname of a remote system

### SSH to R1 from S1.

* + - 1. You must use the **–l** **admin** option when you SSH to R1. This allows you to log in as user **admin**. When prompted, enter **Adm1nP@55** for the password.

S1# **ssh -l admin 192.168.1.1**

Password:

Authorized Users Only!

R1>

* + - 1. You can return to S1 without closing the SSH session to R1 by pressing **Ctrl**+**Shift**+**6**. Release the **Ctrl**+**Shift**+**6** keys and press **x**. The switch privileged EXEC prompt displays.

R1>

S1#

* + - 1. To return to the SSH session on R1, press Enter on a blank CLI line. You may need to press Enter a second time to see the router CLI prompt.

S1#

[Resuming connection 1 to 192.168.1.1 ... ]

R1>

* + - 1. To end the SSH session on R1, type **exit** at the router prompt.

R1# **exit**

[Connection to 192.168.1.1 closed by foreign host]

S1#

#### Question:

What versions of SSH are supported from the CLI?

Type your answers here.

Answers may vary. This can be determined by using the ssh –v ? on the command line. The 2960 switch running IOS version 15.0(2) supports SSH v1 and V2.

S1# ssh -v ?

1 Protocol Version 1

2 Protocol Version 2

Close configuration window

# Reflection Question

How would you provide multiple users, each with their own username, access to a network device?

Type your answers here.

Answers may vary. You would add each user’s username and password to the local database using the username command. It is also possible to use a RADIUS or TACACS server, but this has not been covered yet.

# Router Interface Summary Table

| Router Model | Ethernet Interface #1 | Ethernet Interface #2 | Serial Interface #1 | Serial Interface #2 |
| --- | --- | --- | --- | --- |
| 1800 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 1900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2801 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |
| 2811 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 4221 | Gigabit Ethernet 0/0/0 (G0/0/0) | Gigabit Ethernet 0/0/1 (G0/0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |
| 4300 | Gigabit Ethernet 0/0/0 (G0/0/0) | Gigabit Ethernet 0/0/1 (G0/0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |

**Note**: To find out how the router is configured, look at the interfaces to identify the type of router and how many interfaces the router has. There is no way to effectively list all the combinations of configurations for each router class. This table includes identifiers for the possible combinations of Ethernet and Serial interfaces in the device. The table does not include any other type of interface, even though a specific router may contain one. An example of this might be an ISDN BRI interface. The string in parenthesis is the legal abbreviation that can be used in Cisco IOS commands to represent the interface.

End of document

# Device Configs - Final

# Router R1

service timestamps debug datetime msec

service timestamps log datetime msec

service password-encryption

platform qfp utilization monitor load 80

no platform punt-keepalive disable-kernel-core

!

hostname R1

!

boot-start-marker

boot-end-marker

!

enable secret 5 $1$GCE/$FYYjEAZLjxgbowhYaGm430

!

no aaa new-model

!

no ip domain lookup

ip domain name ccna-lab.com

!

login on-success log

!

subscriber templating

!

multilink bundle-name authenticated

!

no license smart enable

diagnostic bootup level minimal

!

spanning-tree extend system-id

!

username admin secret 5 $1$jamS$qnpkPO7Cr9pSdQxO7nSuQ.

!

redundancy

mode none

!

interface GigabitEthernet0/0/0

no ip address

negotiation auto

!

interface GigabitEthernet0/0/1

ip address 192.168.1.1 255.255.255.0

negotiation auto

!

interface Serial0/1/0

no ip address

!

interface Serial0/1/1

no ip address

!

ip forward-protocol nd

no ip http server

ip http secure-server

!

control-plane

!

banner motd ^C Authorized Users Only ^C

!

line con 0

password 7 094F471A1A0A

logging synchronous

login

transport input none

stopbits 1

line aux 0

stopbits 1

line vty 0 4

password 7 01100F175804

login local

transport input telnet ssh

!

end

# Switch S1

service timestamps debug datetime msec

service timestamps log datetime msec

service password-encryption

!

hostname S1

!

boot-start-marker

boot-end-marker

!

enable secret 5 $1$qwAh$PG.EaIxZQgvrgZtc40Xka0

!

username admin secret 5 $1$vE96$6FO83f1rHurSYktgg2l720

!

no aaa new-model

system mtu routing 1500

no ip domain-lookup

ip domain-name ccna-lab.com

!

spanning-tree mode pvst

spanning-tree extend system-id

!

vlan internal allocation policy ascending

!

interface FastEthernet0/1

!

interface FastEthernet0/2

shutdown

!

interface FastEthernet0/3

shutdown

!

interface FastEthernet0/4

shutdown

!

interface FastEthernet0/5

!

interface FastEthernet0/6

!

interface FastEthernet0/7

shutdown

!

interface FastEthernet0/8

shutdown

!

interface FastEthernet0/9

shutdown

!

interface FastEthernet0/10

shutdown

!

interface FastEthernet0/11

shutdown

!

interface FastEthernet0/12

shutdown

!

interface FastEthernet0/13

shutdown

!

interface FastEthernet0/14

shutdown

!

interface FastEthernet0/15

shutdown

!

interface FastEthernet0/16

shutdown

!

interface FastEthernet0/17

shutdown

!

interface FastEthernet0/18

shutdown

!

interface FastEthernet0/19

shutdown

!

interface FastEthernet0/20

shutdown

!

interface FastEthernet0/21

shutdown

!

interface FastEthernet0/22

shutdown

!

interface FastEthernet0/23

shutdown

!

interface FastEthernet0/24

shutdown

!

interface GigabitEthernet0/1

shutdown

!

interface GigabitEthernet0/2

shutdown

!

interface Vlan1

ip address 192.168.1.11 255.255.255.0

!

ip classless

ip http server

ip http secure-server

!

banner motd ^C Authorized Users Only ^C

!

line con 0

password 7 00071A150754

logging synchronous

login

line vty 0 4

password 7 00071A150754

login local

transport input telnet ssh

line vty 5 15

login

!

end